|  |  |  |  |
| --- | --- | --- | --- |
| **Source** | **Metals Evaluated** | **Environmental Media1** | **IVBA Exposure Pathway Evaluated** |
| Titanium & steel forge | CrVI, total Cr, Co, Mo, Ni, V | Soil and dust | Oral |
| Specialty steel foundry | As, CrVI, total Cr, Co, Ni | Baghouse dust, soil | Oral, Inhalation |
| Steel mill | As, Cd, CrVI, total Cr, Co, Pb, Mn, Ni | EAF and LF slags, furnace dust | Oral, Inhalation |
| Specialty steel forge | Co, Ni | Soil and dust | Oral, Inhalation |
| Steel slag processors | Al, Sb, As, Ba, Be, Cd, Ca, Cr, Co, Cu, Fe, Pb, Mg, Mn, Hg, Mo, Ni, P, Se, Si, Ag, T, Sn, V, Zn | EAF, BOF, and BF slags | Oral |
| Steel slag processor | CrVI, total Cr, Mn | Aged and fresh EAF slag mixed with soil | Oral |